{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":5,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":13,"n_cols":10,"rows_kept":13,"merged":[[0,0,0,9],[2,8,3,8],[8,0,8,5],[8,6,8,9],[9,0,9,9]]}
["2023年“P”项目施工围挡及大门制作安装报价表"]
["序号","物资名称","规格型号","数量","单位","全费用单价限价（元）","供应商所报单价（元）","合计","参考照片","备注"]
[1,"新做定型式彩钢板围挡","围挡采用定型的彩钢材料加工，围挡高度2.5米；镀锌矩管双立柱（50*50*2.5） ；镀锌矩管隔段和边距（30*30*1.2），下部采用不低于 200mm 高黑黄相间的挡浆板，挡浆板采用 0.3mm（厚）×200mm（宽）镀锌钢板，含围挡安装基础。具体做法详见图纸",1900,"米",185]
[2,"新做定型式彩钢板围挡","围挡采用定型的彩钢材料加工，围挡高度2米；镀锌矩管双立柱（50*50*2.5） ；镀锌矩管隔段和边距（30*30*1.2），下部采用不低于 200mm 高黑黄相间的挡浆板，挡浆板采用 0.3mm（厚）×200mm（宽）镀锌钢板，含围挡安装基础。具体做法详见图纸",1900,"米",165]
[3,"喷淋管","PE管",3800,"米",3]
[4,"喷头","不锈钢材质",1300,"个",6]
[6,"电机","功率3000W",20,"个",2600]
[6,"施工大门门头","施工现场出入口设置大门及人工通道，大门门柱和门扇、人工通道颜色为蓝色，字体为白色，门头张贴项目名称，门扇张贴企业名称。门柱采用钢构架体，外包0.5~1mm厚薄钢板，达到美观效果。门扇转动范围内地面必须硬化，表面要平整。大门门柱宽 600mm，进出口宽度6000mm，高度5400mm，门头宽 1000mm，门扇高 2000mm，人工通道宽3000mm，门头左右两侧悬挂五图一牌牌及相关安全标语，具体规格和要求详见图纸。",2,"个",18000]
["合价  （开具税率：                  ）"]
["备注：以上报价均为含税到场安装价；2.要求税率为1%或3%、6%或9%的增值税专票。"]
[{"$nulls":6},"报价单位："]
[{"$nulls":6},"法人或委托代表人及电话："]
[{"$nulls":6},"时间：      年    月     日"]