{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["F.1.1 分部分项工程清单计价表(表-08)【园林绿化工程】"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"F.1.1 分部分项工程清单计价表(表-08)【园林绿化工程】","index":0,"n_rows":111,"n_cols":12,"rows_kept":111,"merged":[[0,0,0,11],[1,0,1,1],[1,2,1,6],[1,7,1,9],[1,10,1,11],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,7],[2,8,3,8],[2,10,2,11],[4,1,4,2],[4,6,4,7],[4,9,4,10],[5,1,5,2],[5,6,5,7],[5,9,5,10],[6,1,6,2],[6,6,6,7],[6,9,6,10],[7,1,7,2],[7,6,7,7],[7,9,7,10],[8,1,8,2],[8,6,8,7],[8,9,8,10],[9,1,9,2],[9,6,9,7],[9,9,9,10],[10,1,10,2],[10,6,10,7],[10,9,10,10],[11,1,11,2],[11,6,11,7],[11,9,11,10],[12,1,12,2],[12,6,12,7],[12,9,12,10],[13,1,13,2],[13,6,13,7],[13,9,13,10],[14,1,14,2],[14,6,14,7],[14,9,14,10],[15,1,15,2],[15,6,15,7],[15,9,15,10],[16,1,16,2],[16,6,16,7],[16,9,16,10],[17,1,17,2],[17,6,17,7],[17,9,17,10],[18,1,18,2],[18,6,18,7],[18,9,18,10],[19,1,19,2],[19,6,19,7],[19,9,19,10],[20,1,20,2],[20,6,20,7],[20,9,20,10],[21,1,21,2],[21,6,21,7],[21,9,21,10],[22,1,22,2],[22,6,22,7],[22,9,22,10],[23,1,23,2],[23,6,23,7],[23,9,23,10],[24,1,24,2],[24,6,24,7],[24,9,24,10],[25,1,25,2],[25,6,25,7],[25,9,25,10],[26,1,26,2],[26,6,26,7],[26,9,26,10],[27,1,27,2],[27,6,27,7],[27,9,27,10],[28,1,28,2],[28,6,28,7],[28,9,28,10],[29,1,29,2],[29,6,29,7],[29,9,29,10],[30,1,30,2],[30,6,30,7],[30,9,30,10],[31,1,31,2],[31,6,31,7],[31,9,31,10],[32,1,32,2],[32,6,32,7],[32,9,32,10],[33,1,33,2],[33,6,33,7],[33,9,33,10],[34,1,34,2],[34,6,34,7],[34,9,34,10],[35,1,35,2],[35,6,35,7],[35,9,35,10],[36,1,36,2],[36,6,36,7],[36,9,36,10],[37,1,37,2],[37,6,37,7],[37,9,37,10],[38,1,38,2],[38,6,38,7],[38,9,38,10],[39,1,39,2],[39,6,39,7],[39,9,39,10],[40,1,40,2],[40,6,40,7],[40,9,40,10],[41,1,41,2],[41,6,41,7],[41,9,41,10],[42,1,42,2],[42,6,42,7],[42,9,42,10],[43,1,43,2],[43,6,43,7],[43,9,43,10],[44,1,44,2],[44,6,44,7],[44,9,44,10],[45,1,45,2],[45,6,45,7],[45,9,45,10],[46,1,46,2],[46,6,46,7],[46,9,46,10],[47,1,47,2],[47,6,47,7],[47,9,47,10],[48,1,48,2],[48,6,48,7],[48,9,48,10],[49,1,49,2],[49,6,49,7],[49,9,49,10],[50,1,50,2],[50,6,50,7],[50,9,50,10],[51,1,51,2],[51,6,51,7],[51,9,51,10],[52,1,52,2],[52,6,52,7],[52,9,52,10],[53,1,53,2],[53,6,53,7],[53,9,53,10],[54,1,54,2],[54,6,54,7],[54,9,54,10],[55,1,55,2],[55,6,55,7],[55,9,55,10],[56,1,56,2],[56,6,56,7],[56,9,56,10],[57,1,57,2],[57,6,57,7],[57,9,57,10],[58,1,58,2],[58,6,58,7],[58,9,58,10],[59,1,59,2],[59,6,59,7],[59,9,59,10],[60,1,60,2],[60,6,60,7],[60,9,60,10],[61,1,61,2],[61,6,61,7],[61,9,61,10],[62,1,62,2],[62,6,62,7],[62,9,62,10],[63,1,63,2],[63,6,63,7],[63,9,63,10],[64,1,64,2],[64,6,64,7],[64,9,64,10],[65,1,65,2],[65,6,65,7],[65,9,65,10],[66,1,66,2],[66,6,66,7],[66,9,66,10],[67,1,67,2],[67,6,67,7],[67,9,67,10],[68,1,68,2],[68,6,68,7],[68,9,68,10],[69,1,69,2],[69,6,69,7],[69,9,69,10],[70,1,70,2],[70,6,70,7],[70,9,70,10],[71,1,71,2],[71,6,71,7],[71,9,71,10],[72,1,72,2],[72,6,72,7],[72,9,72,10],[73,1,73,2],[73,6,73,7],[73,9,73,10],[74,1,74,2],[74,6,74,7],[74,9,74,10],[75,1,75,2],[75,6,75,7],[75,9,75,10],[76,1,76,2],[76,6,76,7],[76,9,76,10],[77,1,77,2],[77,6,77,7],[77,9,77,10],[78,1,78,2],[78,6,78,7],[78,9,78,10],[79,1,79,2],[79,6,79,7],[79,9,79,10],[80,1,80,2],[80,6,80,7],[80,9,80,10],[81,1,81,2],[81,6,81,7],[81,9,81,10],[82,1,82,2],[82,6,82,7],[82,9,82,10],[83,1,83,2],[83,6,83,7],[83,9,83,10],[84,1,84,2],[84,6,84,7],[84,9,84,10],[85,1,85,2],[85,6,85,7],[85,9,85,10],[86,1,86,2],[86,6,86,7],[86,9,86,10],[87,1,87,2],[87,6,87,7],[87,9,87,10],[88,1,88,2],[88,6,88,7],[88,9,88,10],[89,1,89,2],[89,6,89,7],[89,9,89,10],[90,1,90,2],[90,6,90,7],[90,9,90,10],[91,1,91,2],[91,6,91,7],[91,9,91,10],[92,1,92,2],[92,6,92,7],[92,9,92,10],[93,1,93,2],[93,6,93,7],[93,9,93,10],[94,1,94,2],[94,6,94,7],[94,9,94,10],[95,1,95,2],[95,6,95,7],[95,9,95,10],[96,1,96,2],[96,6,96,7],[96,9,96,10],[97,1,97,2],[97,6,97,7],[97,9,97,10],[98,1,98,2],[98,6,98,7],[98,9,98,10],[99,1,99,2],[99,6,99,7],[99,9,99,10],[100,1,100,2],[100,6,100,7],[100,9,100,10],[101,1,101,2],[101,6,101,7],[101,9,101,10],[102,1,102,2],[102,6,102,7],[102,9,102,10],[103,1,103,2],[103,6,103,7],[103,9,103,10],[104,1,104,2],[104,6,104,7],[104,9,104,10],[105,1,105,2],[105,6,105,7],[105,9,105,10],[106,1,106,2],[106,6,106,7],[106,9,106,10],[107,1,107,2],[107,6,107,7],[107,9,107,10],[108,1,108,2],[108,6,108,7],[108,9,108,10],[109,1,109,2],[109,6,109,7],[109,9,109,10],[110,0,110,8],[110,9,110,10]],"flags":["formulas_cached_only"]}
["机场路景观改造提升工程苗木移植（第一标段）工程量清单与报价表","","","","","","","","","","",""]
["工程名称：","","机场路景观改造提升工程苗木移植（第一标段）","","","","",null,"",""," ",""]
["序号","项目编码","","项目名称","项目特征描述","计量\r\n单位","工程量","","全费用单价限价(元)","","金额（元）"]
["","","","","","","","",null,"合价","全费用单价","合  计"]
[" "," ","","机场路移植玉带河公园"," "," "," ",""," "," ",""," "]
["1","050102001001","","移植广玉兰3-4","1.乔木种类：移植广玉兰\r\n2.乔木规格：(胸径3-4cm)\r\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","128","","60.95",null,null,""]
["2","050102001002","","移植广玉兰5","1.乔木种类：移植广玉兰\r\n2.乔木规格：(胸径5cm)\r\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","53","","60.95",null,null,""]
["3","050102001003","","移植广玉兰6-8","1.乔木种类：移植广玉兰\n2.乔木规格：(胸径6-8cm)\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标\n人自行考虑\n4.养护：100%成活率；养护期一\n年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。","株","72","","84.59",null,null,""]
["4","050102001004","","移植贞楠3-4","1.乔木种类：移植贞楠\r\n2.乔木规格：(胸径3-4cm)\r\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","5","","56.07",null,null,""]
["5","050102001005","","移植贞楠5-6","1.乔木种类：移植贞楠\n2.乔木规格：(胸径5-6cm)\n3.场内外运输方式及运输距离：\n石洞机场路至玉带河公园，投标\n人自行考虑\n4.养护：100%成活率；养护期一年                                                                                                            5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。\r","株","8","","77.80",null,null,""]
["6","050102001006","","移植贞楠7","1.乔木种类：移植贞楠\r\n2.乔木规格：(胸径7cm)\r\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","91","","77.80",null,null,""]
["7","050102001007","","移植天竺葵2-3","1.乔木种类：移植天竺桂\n2.乔木规格：(胸径2-3cm)\n3.场内外运输方式及运输距离: \n石洞机场路至玉带河公园，投标\n人自行考虑\n4.养护：100%成活率；养护期一\n年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质                                                                                                           量、施工验收规范要求。","株","25","","56.41",null,null,""]
["8","050102001008","","移植蓝花楹5-6","1.乔木种类：移植蓝花楹\r\n2.乔木规格：(胸径5-6cm)\r\n3.场内外运输方式及运输距离： 石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","15","","71.80",null,null,""]
["9","050102001009","","移植蓝花楹6-8","1.乔木种类：移植蓝花楹\r\n2.乔木规格：(胸径6-8cm)\r\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","181","","84.58",null,null,""]
["10","050102001010","","移植蓝花楹10-12","1.乔木种类：移植蓝花楹\n2.乔木规格：(胸径10-12cm)\n3.场内外运输方式及运输距离：                                                                                                             石洞机场路至玉带河公园，投标\n人自行考虑\n4.养护：100%成活率；养护期一\n年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。","株","28","","174.97",null,null,""]
["11","050102001011","","移植白玉兰2-4","1.乔木种类：移植广玉兰\r\n2.乔木规格：(胸径2-4cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","20","","60.95",null,null,""]
["12","050102001012","","移植碧桃6-8","1.乔木种类：移植蓝花楹\n2.乔木规格：(胸径6-8cm)\n3.场内外运输方式及运输距离：\n石洞机场路至玉带河公园，投标\n人自行考虑\n4.养护：100%成活率；养护期一年                                                                                                           5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。\r","株","78","","84.58",null,null,""]
["13","050102002013","","移植桂花4-5","1.乔木种类：移植桂花\r\n2.胸径:4-5cm\r\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","22","","55.41",null,null,""]
["14","050102002014","","移植桂花6-7","1.乔木种类：移植桂花\n2.胸径：6-7cm\n3.场内外运输方式及运输距离： \n石洞机场路至玉带河公园，投标\n人自行考虑\n4.养护：100%成活率；养护期一\n年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质                                                                                                             量、施工验收规范要求。","株","49","","84.40",null,null,""]
["15","050102002015","","移植桂花8","1.乔木种类：移植桂花\r\n2.胸径：8cm\r\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","23","","138.93",null,null,""]
["16","050102001016","","移植栾树1-4","1.乔木种类：移植栾树\r\n2.乔木规格：(胸径1-4cm)\r\n3.场内外运输方式及运输距离： 石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","244","","60.95",null,null,""]
["17","050102001017","","移植栾树5-6\r\n-6","1.乔木种类：移植栾树\n2.乔木规格：(胸径5-6cm)\n3.场内外运输方式及运输距离：                                                                                                             石洞机场路至玉带河公园，投\n标人自行考虑\n4.养护：100%成活率；养护期一\n年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。\r","株","425","","84.58",null,null,""]
["18","050102001018","","移植栾树6-8","1.乔木种类：移植栾树\r\n2.乔木规格：(胸径6-8cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","65","","140.88",null,null,""]
["19","050102001019","","移植栾树8-9","1.乔木种类：移植栾树\n2.乔木规格：(胸径8-9cm)\n3.场内外运输方式及运输距离：\n石洞机场路至玉带河公园，投标\n人自行考虑\n4.养护：100%成活率；养护期一年                                                                                                            5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。\r","株","463","","140.88",null,null,""]
["20","050102001020","","移植栾树10-15","1.乔木种类：移植栾树\r\n2.乔木规格：(胸径10-15cm)\r\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","244","","228.43",null,null,""]
["21","050102001021","","移植羊蹄甲4-5","1.乔木种类：移植羊蹄甲\n2.乔木规格：(胸径4-5cm)\n3.场内外运输方式及运输距离：\n石洞机场路至玉带河公园，投标\n人自行考虑\n4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质                                                                                                           量、施工验收规范要求。","株","44","","60.95",null,null,""]
["22","050102001022","","移植羊蹄甲6-8","1.乔木种类：移植羊蹄甲\r\n2.乔木规格：(胸径6-8cm)\r\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","226","","84.59",null,null,""]
["23","050102001023","","移植羊蹄甲8-10","1.乔木种类：移植羊蹄甲\r\n2.乔木规格：(胸径8-10cm)\r\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","25","","103.69",null,null,""]
["24","050102001024","","移植羊蹄甲15-20\r\n","1.乔木种类：移植羊蹄甲\n2.乔木规格：(胸径15-20cm)\n3.场内外运输方式及运输距离：                                                                                                             石洞机场路至玉带河公园，投标\n人自行考虑\n4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。","株","3","","506.06",null,null,""]
["25","050102001025","","移植羊蹄甲35-40","1.乔木种类：移植羊蹄甲\r\n2.乔木规格：(胸径35-40cm)\r\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","7","","1461.41",null,null,""]
["26","050102001026","","移植小叶榕8-10","1.乔木种类：移植小叶榕\n2.乔木规格：(胸径8-10cm)\n3.场内外运输方式及运输距离：\n  石洞机场路至玉带河公园，投\n标人自行考虑\n4.养护：100%成活率；养护期一年                                                                                                            5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。\r","株","32","","75.17",null,null,""]
["27","050102001027","","移植小叶榕10-12","1.乔木种类：移植小叶榕\r\n2.乔木规格：(胸径10-12cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","45","","125.34",null,null,""]
["28","050102001028","","移植小叶榕13-17","1.乔木种类：移植小叶榕\n2.乔木规格：(胸径13-17cm)\n3.场内外运输方式及运输距离：\n  石洞机场路至玉带河公园，投\n标人自行考虑\n4.养护：100%成活率；养护期一\n年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质量、施工验收规范要求。","株","53","","225.85",null,null,""]
["29","050102001029","","移植萍婆丛生","1.乔木种类：移植萍婆\r\n2.乔木规格：丛生\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","16","","77.81",null,null,""]
["30","050102001030","","移植杨梅17-22","1.乔木种类：移植杨梅\r\n2.乔木规格：(胸径17-22cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","3","","369.38",null,null,""]
["31","050102002031","","移植紫荆12","1.灌木种类：移植紫荆\n2.地径：12cm\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\n4.养护：100%成活率；养护期一年\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","1","","70.97",null,null,""]
["32","050102002032","","移植丛生紫薇3-6","1.灌木种类：移植紫薇\r\n2.地径：3-6cm\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","69","","58.49",null,null,""]
["33","050102002033","","移植丛生紫薇8-10","1.灌木种类：移植紫薇\r\n2.地径：8-10cm\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","2","","72.76",null,null,""]
["34","050102001034","","移植黄角树12-15","1.乔木种类：移植黄角树                                                                                                                    2.乔木规格：(胸径12-15cm)\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\n4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工规范要求\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。\r","株","3","","115.52",null,null,""]
["35","050102002035","","移植红花继木球冠幅80","1.灌木种类：移植红继木球\r\n2.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n3.养护：100%成活率；养护期一年\r\n4.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","32","","44.22",null,null,""]
["36","050102001036","","移植蒲葵高度35-50","1.乔木种类：移植蒲葵\n2.乔木规格：(胸径35-50cm)\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\n4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工规范要求\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","64","","1943.61",null,null,""]
["37","050102001037","","移植三叶树12-15","1.乔木种类：移植黄角树\r\n2.乔木规格：(胸径12-15cm)\r\n3.场内外运输方式及运输距离：\r\n 石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","7","","103.77",null,null,""]
["38","050102002038","","移植万年青球高80","1.灌木种类：移植万年球\r\n2.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n3.养护：100%成活率；养护期一年\r\n4.做法：不允许随意修剪，满足设计及现行技术、质量、施工验收规范要求。","株","7","","16.11",null,null,""]
["39","050102002039","","移植银杏2-5","1.种类：移植白果银杏2-5cm\n2.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\n3.养护：100%成活率；养护期一年\n4.草绳绕树干、支撑：符合施工规范要求\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","27","","36.24",null,null,""]
["40","050102002040","","移植单杆红叶石楠5-7","1.种类：移植单杆红叶石楠5-7cm\r\n2.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n3.养护：100%成活率；养护期一年\r\n4.草绳绕树干、支撑：符合施工规范要求\r\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","62","","52.45",null,null,""]
["41","050102001041","","移植栾树苗","1.乔木种类：移植栾树苗\n2.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\n3.养护：100%成活率；养护期一年\n4.草绳绕树干、支撑：符合施工规范要求                                                                                                                                  5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。\r","株","152","","66.06",null,null,""]
["42","050102001042","","移植栾树2-9","1.乔木种类：移植栾树\r\n2.乔木规格：(胸径2-9cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","1684","","105.45",null,null,""]
["43","050102001043","","移植栾树10-14","1.乔木种类：移植栾树\r\n2.乔木规格：(胸径10-14cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","1727","","174.13",null,null,""]
["44","050102001044","","移植蓝花楹4-9","1.乔木种类：移植蓝花楹                                                                                                                      2.乔木规格：(胸径4-9cm)\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\n4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工规范要求\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。\r","株","887","","78.19",null,null,""]
["45","050102001045","","移植蓝花楹10-17","1.乔木种类：移植蓝花楹\r\n2.乔木规格：(胸径10-17cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","514","","275.48",null,null,""]
["46","050102001046","","移植蓝花楹18-19","1.乔木种类：移植蓝花楹\n2.乔木规格：(胸径18-19cm)\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑                                                                                                                             4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工规范要求\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。\r","株","10","","375.23",null,null,""]
["47","050102002047","","移植银杏3-6\r\n银杏3-6","1.种类：移植白果银杏3-6cm\r\n2.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n3.养护：100%成活率；养护期一年\r\n4.草绳绕树干、支撑：符合施工规范要求\r\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","83","","36.24",null,null,""]
["48","050102001048","","移植羊蹄甲3-10","1.乔木种类：移植羊蹄甲\n2.乔木规格：(胸径3-10cm)\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\n4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工规范要求\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","513","","78.19",null,null,""]
["49","050102001049","","移植羊蹄甲11-19","1.乔木种类：移植羊蹄甲\r\n2.乔木规格：(胸径11-19cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","255","","265.32",null,null,""]
["50","050102001050","","移植羊蹄甲20-39","1.乔木种类：移植羊蹄甲\r\n2.乔木规格：(胸径20-39cm)\r\n3.场内外运输方式及运输距离：\r\n石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","274","","891.80",null,null,""]
["51","050102001051","","移植羊蹄甲40-63","1.乔木种类：移植羊蹄甲\n2.乔木规格：(胸径40-63cm)                                                                                                                 3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\n4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工规范要求\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。\r","株","18","","1476.33",null,null,""]
["52","050102002052","","移植红叶石楠球5-6","1.灌木种类：移植红叶石楠球5-6\r\n2.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n3.养护：100%成活率；养护期一年\r\n4.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","1204","","45.93",null,null,""]
["53","050102002053","","移植桂花3-8","1.乔木种类：移植桂花\n2.胸径:3-8cm\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\n4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工规范要求                                                                                                                                  6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。\r","株","490","","45.18",null,null,""]
["54","050102002054","","移植桂花9-15","1.乔木种类：移植桂花\r\n2.胸径：9-15cm\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","115","","123.27",null,null,""]
["55","050102001055","","移植桂花25","1.乔木种类：移植桂花\r\n2.乔木规格：(胸径25cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","1","","1000.64",null,null,""]
["56","050102001056","","移植天竺桂苗","1.乔木种类：移植天竺桂苗                                                                                                                 2.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\n3..养护：100%成活率；养护期一年\n4.草绳绕树干、支撑：符合施工规范要求\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。\r","株","213","","62.09",null,null,""]
["57","050102001057","","移植天竺桂10-12","1.乔木种类：移植天竺桂10-12 \r\n2.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n3.养护：100%成活率；养护期一年\r\n4.草绳绕树干、支撑：符合施工规范要求\r\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","18","","132.67",null,null,""]
["58","050102001058","","移植天竺桂12-20","1.乔木种类：移植天竺桂12-20\n2.场内外运输方式及运输距离：\n  石洞机场路至玉带河公园，投\n标人自行考虑\n3.养护：100%成活率；养护期一年\n4.草绳绕树干、支撑：符合施工规范要求\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","25","","345.04",null,null,""]
["59","050102001059","","移植香樟3-8","1.乔木种类：移植香樟\r\n2.乔木规格：(胸径3-8cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","2","","100.41",null,null,""]
["60","050102001060","","移植香樟16-42","1.乔木种类：移植香樟\r\n2.乔木规格：(胸径16-42cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","45","","668.48",null,null,""]
["61","050102001061","","移植广玉兰7-10","1.乔木种类：移植广玉兰\r\n2.乔木规格：(胸径5-8cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","700","","145.48",null,null,""]
["62","050102002062","","移植海桐球冠幅50-70","1.灌木种类：移植海桐球  冠幅50-70\r\n2.场内外运输方式及运输距离： 石洞机场路运至玉带河公园，投标人自行考虑\r\n3.养护：100%成活率；养护期一年\r\n4.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","882","","23.53",null,null,""]
["63","050102001063","","移植杨梅16-22","1.乔木种类：移植杨梅\r\n2.乔木规格：(胸径16-22cm)\r\n3.场内外运输方式及运输距离：\r\n石洞机场路运至玉带河公园，投\r\n标人自行考虑\r\n4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。","株","7","","372.83",null,null,""]
["64","050102001064","","移植萍婆7-9","1.乔木种类：移植萍婆\r\n2.乔木规格：(胸径7-9cm)\r\n3.场内外运输方式及运输距离：石洞机场路运至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","20","","78.06",null,null,""]
["65","050102001065","","移植萍婆15","1.乔木种类：移植萍婆\n2.乔木规格：(胸径15cm)\n3.场内外运输方式及运输距离：\n石洞机场路运至玉带河公园，投\n标人自行考虑\n4.养护：100%成活率；养护期一\n年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","31","","226.97",null,null,""]
["66","050102002066","","移植紫薇8-10","1.灌木种类：移植紫薇\r\n2.地径:8-10cm\r\n3.场内外运输方式及运输距离：石洞机场路运至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","47","","38.65",null,null,""]
["67","050102002067","","移植紫薇22","1.灌木种类：移植紫薇\r\n2.地径：22cm\r\n3.场内外运输方式及运输距离：石洞机场路运至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","1","","330.36",null,null,""]
["68","050102002068","","移植白玉兰5-8","1.灌木种类：移植紫玉兰\n2.地径：5-8cm\n3.场内外运输方式及运输距离：\n石洞机场路运至玉带河公园，投\n标人自行考虑\n4.养护：100%成活率；养护期一年\n5.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。","株","28","","20.00",null,null,""]
["69","050102001069","","移植红枫3-6","1.乔木种类：移植红枫\r\n2.乔木规格：(胸径3-6cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","24","","60.33",null,null,""]
["70","050102001070","","移植红枫14","1.乔木种类：移植红枫\r\n2.乔木规格：(胸径14cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","1","","251.96",null,null,""]
["71","050102002071","","移植紫玉兰3-8","1.灌木种类：移植紫玉兰\r\n2.地径：3-8cm\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","235","","37.42",null,null,""]
["72","050102002072","","移植万年青球冠幅50-70","1.灌木种类：移植万年青球冠幅50-70\r\n2.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n3.养护：100%成活率；养护期一年\r\n4.做法：不允许随意修剪，满足设计及现行技术、质量、施工验收规范要求。","株","526","","16.11",null,null,""]
["73","050102002073","","移植红花继木球冠幅60-80","1.灌木种类：移植红花继木球冠\n幅60-80\n2.场内外运输方式及运输距离：\n  石洞机场路至玉带河公园，投\n标人自行考虑\n3.养护：100%成活率；养护期一年\n4.做法：全树冠（不允许随意修剪），满足设计及现行技术、质\n量、施工验收规范要求。","株","246","","14.84",null,null,""]
["74","050102001074","","移植贞楠5-9","1.乔木种类：移植贞楠\r\n2.乔木规格：(胸径5-9cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","56","","71.32",null,null,""]
["75","050102001075","","移植贞楠19","1.乔木种类：移植贞楠\r\n2.乔木规格：(胸径19cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","1","","372.09",null,null,""]
["76","050102001076","","移植重阳木11-16","1.乔木种类：移植重阳木\n2.乔木规格：(胸径11-16cm)                                                                                                                           3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\n4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工规范要求\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。\r","株","130","","195.33",null,null,""]
["77","050102002077","","移植栀子花冠幅20-40","1.灌木种类：移植栀子花冠幅20-40\r\n2.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n3.养护：100%成活率；养护期一年\r\n4.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","613","","13.19",null,null,""]
["78","050102002078","","移植地笼桂冠幅80-120","1.灌木种类：移植地笼桂冠幅80-\n120\n2.场内外运输方式及运输距离：\n  石洞机场路至玉带河公园，投\n标人自行考虑\n3.养护：100%成活率；养护期一年\n4.草绳绕树干、支撑：符合施工规范要求\n5.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。","株","646","","44.24",null,null,""]
["79","050102001079","","移植池衫8","1.乔木种类：移植池衫\r\n2.乔木规格：(胸径8cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","42","","90.73",null,null,""]
["80","050102002080","","移植紫荆4-7","1.灌木种类：移植紫荆\r\n2.地径：4-7cm\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","6","","27.26",null,null,""]
["81","050102001081","","移植小叶榕8-19","1.乔木种类：移植小叶榕\n2.乔木规格：(胸径8-19cm)                                                                                                                       3.场内外运输方式及运输距离：\n 石洞机场路至玉带河公园，投标\n人自行考虑\n4.养护：100%成活率；养护期一\n年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。\r","株","78","","269.27",null,null,""]
["82","050102001082","","移植小叶榕20-29","1.乔木种类：移植小叶榕\r\n2.乔木规格：(胸径20-29cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","50","","783.79",null,null,""]
["83","050102001083","","移植小叶榕30-45","1.乔木种类：移植小叶榕\n2.乔木规格：(胸径30-45cm)\n3.场内外运输方式及运输距离：\n  石洞机场路至玉带河公园，投\n标人自行考虑\n4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。","株","8","","1337.12",null,null,""]
["84","050102002084","","移植三角梅","1.灌木种类：移植三角梅\r\n2.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n3.养护：100%成活率；养护期一年\r\n4.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","339","","13.20",null,null,""]
["85","050102001085","","移植红千层6-10","1.乔木种类：移植红千层\r\n2.乔木规格：(胸径6-10cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","60","","77.90",null,null,""]
["86","050102002086","","移植红千层12-14","1.乔木种类：移植红千层                                                                                                                            2.乔木规格：(胸径12-14cm)\n3.场内外运输方式及运输距离：\n  石洞机场路至玉带河公园，投\n标人自行考虑\n4..养护：100%成活率；养护期\n一年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。\r","株","25","","184.46",null,null,""]
["87","050102001087","","移植蒲葵高度35-50","1.乔木种类：移植蒲葵\r\n2.乔木规格：(胸径35-50cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","44","","1943.61",null,null,""]
["88","050102001088","","移植角斛树34","1.乔木种类：移植角斛树\n2.乔木规格：(胸径34cm)\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑                                                                                                                                      4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工规范要求\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。\r","株","1","","1345.85",null,null,""]
["89","050102002089","","移植红豆杉9-10","1.乔木种类：移植红豆杉\r\n2.乔木规格：(胸径9-10cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","8","","78.14",null,null,""]
["90","050102001090","","移植国槐树14-27","1.乔木种类：移植国槐树\n2.乔木规格：(胸径14-27cm)\n3.场内外运输方式及运输距离：石洞机场路至玉带河公园，投标人自行考虑\n4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工规范要求                                                                                                                                      6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。\r","株","19","","809.66",null,null,""]
["91","050102001091","","移植角斛树30-40","1.乔木种类：移植角斛树\r\n2.乔木规格：(胸径30-40cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","23","","1254.92",null,null,""]
["92","050102001092","","移植加那利海藻高度40-60","1.乔木种类：移植加那利海藻高度40-60\r\n2.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n3.养护：100%成活率；养护期一年\r\n4.草绳绕树干、支撑：符合施工规范要求\r\n5.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","27","","53.63",null,null,""]
["93","050102001093","","移植中东海藻高度40-60","1.乔木种类：移植中东海枣高度40-60\n2.场内外运输方式及运输距离：\n  石洞机场路至玉带河公园，投\n标人自行考虑\n3.养护：100%成活率；养护期一\n年\n4.草绳绕树干、支撑：符合施工\n规范要求\n5.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。","株","66","","56.04",null,null,""]
["94","050102001094","","移植朴树14-26","1.乔木种类：移植朴树\r\n2.乔木规格：(胸径14-26cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","5","","367.72",null,null,""]
["95","050102001095","","移植朴树35-84","1.乔木种类：移植朴树\n2.乔木规格：(胸径35-84cm)\n3.场内外运输方式及运输距离：\n  石洞机场路至玉带河公园，投\n标人自行考虑                                                                                                                               4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。\r","株","308","","1511.14",null,null,""]
["96","050102001096","","移植刺桐40","1.乔木种类：移植刺桐\r\n2.乔木规格：(胸径40cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","24","","1420.50",null,null,""]
["97","050102001097","","移植刺桐53","1.乔木种类：移植刺桐\n2.乔木规格：(胸径53cm)\n3.场内外运输方式及运输距离：\n  石洞机场路至玉带河公园，投\n标人自行考虑\n4.养护：100%成活率；养护期一\n年\n5.草绳绕树干、支撑：符合施工\n规范要求                                                                                                                                          6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质\n量、施工验收规范要求。\r","株","6","","1451.27",null,null,""]
["98","050102001098","","移植鸡冠刺桐10-15","1.乔木种类：移植鸡冠刺桐\r\n2.乔木规格：(胸径10-15cm)\r\n3.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","20","","201.09",null,null,""]
["99","050102001099","","移植红花继木桩高度180","1.灌木种类：移植红花继木桩高度180\r\n2.场内外运输方式及运输距离：\r\n  石洞机场路至玉带河公园，投标人自行考虑\r\n3.养护：100%成活率；养护期一年\r\n4.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","31","","49.73",null,null,""]
["100","050102001100","","移植多头香樟地径70-120","1.乔木种类：移植香樟\n2.乔木规格：(胸径70-120cm)\n3.场内外运输方式及运输距离：石洞机场路运至玉带河公园，投\n标人自行考虑\n4.养护：100%成活率；养护期一年\n5.草绳绕树干、支撑：符合施工规范要求\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","6","","1429.36",null,null,""]
["101","050102001101","","移植多宝树地径70-120","1.乔木种类：移植多宝树\r\n2.乔木规格：胸径70-120cm\r\n3.场内外运输方式及运输距离：石洞机场路运至玉带河公园，投标人自行考虑\r\n4.养护：100%成活率；养护期一年\r\n5、草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","10","","1675.16",null,null,""]
["102","050102001102","","移植红叶李6","1.乔木种类：移植广玉兰\n2.乔木规格：(胸径6cm)\n3.场内外运输方式及运输距离：\n石洞机场路运至玉带河公园，投\n标人自行考虑\n4.养护：100%成活率；养护期一年                                                                                                                5.草绳绕树干、支撑：符合施工规范要求\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。\r","株","1","","84.59",null,null,""]
["103","050102001103","","移植黄角树48-64","1.乔木种类：移植黄角树\r\n2.乔木规格：(胸径48-64cm)\r\n3.场内外运输方式及运输距离：石洞机场路运至玉带河公园，投标人自行考虑\r\n4..养护：100%成活率；养护期一年\r\n5.草绳绕树干、支撑：符合施工规范要求\r\n6.做法：全树冠（不允许随意修剪），满足设计及现行技术、质量、施工验收规范要求。","株","13","","1463.56",null,null,""]
[104,"050102001104","","移植黄角树87-175","1.乔木种类：移植黄角树\n2.乔木规格：胸径87cm-175cm\n3.场内外运输方式及运输距离：\n石洞机场路运至玉带河公园，投\n标人自行考虑\n4..养护：100%成活率；养护期\n一年\n5.草绳绕树干、支撑：符合施工\n规范要求\n6.做法：全树冠（不允许随意修\n剪），满足设计及现行技术、质量、施工验收规范要求。","株","2","","2120.98",null,null,""]
["105","050102008105","","移植麦冬","1.地被种类：移植麦冬\r\n2.场内外运输方式及运输距离：石洞机场路运至玉带河公园，投标人自行考虑\r\n3.养护：100%成活率；养护期一年\r\n6.做法：不允许随意修剪，满足设计及现行技术、质量、施工验收规范要求。","m2","200","","24.42",null,null,""]
["合　　计","","","","","","","","",null,"",""]