{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["安装工程"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"安装工程","index":0,"n_rows":50,"n_cols":12,"rows_kept":50,"merged":[[0,0,0,11],[1,0,1,1],[1,2,1,6],[1,7,1,9],[1,10,1,11],[2,0,3,0],[2,1,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,7],[2,8,3,8],[2,10,2,11],[4,1,4,2],[4,6,4,7],[4,9,4,10],[5,1,5,2],[5,6,5,7],[5,9,5,10],[6,1,6,2],[6,6,6,7],[6,9,6,10],[7,1,7,2],[7,6,7,7],[7,9,7,10],[8,1,8,2],[8,6,8,7],[8,9,8,10],[9,1,9,2],[9,6,9,7],[9,9,9,10],[10,1,10,2],[10,6,10,7],[10,9,10,10],[11,1,11,2],[11,6,11,7],[11,9,11,10],[12,1,12,2],[12,6,12,7],[12,9,12,10],[13,1,13,2],[13,6,13,7],[13,9,13,10],[14,1,14,2],[14,6,14,7],[14,9,14,10],[15,1,15,2],[15,6,15,7],[15,9,15,10],[16,1,16,2],[16,6,16,7],[16,9,16,10],[17,1,17,2],[17,6,17,7],[17,9,17,10],[18,1,18,2],[18,6,18,7],[18,9,18,10],[19,1,19,2],[19,6,19,7],[19,9,19,10],[20,1,20,2],[20,6,20,7],[20,9,20,10],[21,1,21,2],[21,6,21,7],[21,9,21,10],[22,1,22,2],[22,6,22,7],[22,9,22,10],[23,1,23,2],[23,6,23,7],[23,9,23,10],[24,1,24,2],[24,6,24,7],[24,9,24,10],[25,1,25,2],[25,6,25,7],[25,9,25,10],[26,1,26,2],[26,6,26,7],[26,9,26,10],[27,1,27,2],[27,6,27,7],[27,9,27,10],[28,1,28,2],[28,6,28,7],[28,9,28,10],[29,1,29,2],[29,6,29,7],[29,9,29,10],[30,1,30,2],[30,6,30,7],[30,9,30,10],[31,1,31,2],[31,6,31,7],[31,9,31,10],[32,1,32,2],[32,6,32,7],[32,9,32,10],[33,1,33,2],[33,6,33,7],[33,9,33,10],[34,1,34,2],[34,6,34,7],[34,9,34,10],[35,1,35,2],[35,6,35,7],[35,9,35,10],[36,1,36,2],[36,6,36,7],[36,9,36,10],[37,1,37,2],[37,6,37,7],[37,9,37,10],[38,1,38,2],[38,6,38,7],[38,9,38,10],[39,1,39,2],[39,6,39,7],[39,9,39,10],[40,1,40,2],[40,6,40,7],[40,9,40,10],[41,1,41,2],[41,6,41,7],[41,9,41,10],[42,1,42,2],[42,6,42,7],[42,9,42,10],[43,1,43,2],[43,6,43,7],[43,9,43,10],[44,1,44,2],[44,6,44,7],[44,9,44,10],[45,1,45,2],[45,6,45,7],[45,9,45,10],[46,1,46,2],[46,6,46,7],[46,9,46,10],[47,1,47,2],[47,6,47,7],[47,9,47,10],[48,1,48,2],[48,6,48,7],[48,9,48,10],[49,0,49,8],[49,9,49,11]],"flags":["formulas_cached_only"]}
["机场路景观改造提升工程给水安装工程量清单与报价表","","","","","","","","","","",""]
["工程名称：","","机场路景观改造提升工程（喷灌系统）","","","","",null,"","","",""]
["序号","项目编码","","项目名称","项目特征描述","计量\r\n单位","工程量","","全费用单价限价(元)","","金额（元）"]
["","","","","","","","",null,"合价","全费用单价","合  计"]
[" "," ","","土建工程"," "," "," ",""," "," ",""," "]
["1","040504001001","","VB-708阀门箱安装","1.垫层、基础材质及厚度：C15砼垫层 厚100mm\r\n2.砌筑材料品种、规格、强度等级 MN10砖 内空：300*300*500\r\n3.勾缝、抹面要求 ：内1：2水泥砂浆抹面\r\n4.砂浆强度等级、配合比 ：M7.5\r\n5.混凝土强度等级 C15\r\n6.其他：未尽事宜满足设计及现行技术、质量验收规范要求","座","613","","259.76",null,null,""]
["2","040504001002","","1220门箱安装","1.垫层、基础材质及厚度：C15砼垫层 厚100mm\r\n2.砌筑材料品种、规格、强度等级 MN10砖 内空1.6*0.6\r\n3.勾缝、抹面要求 ：内1：2水泥砂浆抹面\r\n4.砂浆强度等级、配合比 ：M7.5\r\n5.混凝土强度等级 C15\r\n6.盖板材质、规格 :塑料\r\n7.井盖、井圈材质及规格 塑料\r\n8.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","座","186","","402.15",null,null,""]
["3","040101002003","","挖沟槽土石方","1.土壤类别及开挖方式 ：投标人踏勘现场后自行考虑开挖方式及土石比例\r\n2.挖土深度：按设计及规范要求\r\n3.其他：未尽事宜满足设计及现行技术、质量验收规范要求","m3","18000","","14.59",null,null,""]
["4","040101002003","","挖沟槽土石方（人工）","1.人工挖沟槽土石方 ：在遇到机械无法施工或地下管线等无法使用机械开挖时，选择人工挖土石方。\r\n2.挖土深度：按设计及规范要求\r\n3.其他：未尽事宜满足设计及现行技术、质量验收规范要求","m3","2000","","25.17",null,null,""]
["5","040103001036","","回填方","1.密实度要求 ：按设计及规范要求\r\n2.填方材料品种 ：按设计及规范要求\r\n3.填方粒径要求 ：按设计及规范要求\r\n4.填方来源、运距：投标单位自行考虑\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求","m3","13000","","10.45",null,null,""]
["6","040305001005","","管沟砂垫层","1.材料品种：规格 详设计图\r\n2.厚度：100mm\r\n3.其他：未尽事宜满足设计及现行技术、质量验收规范要求","m3","3000","","103.68",null,null,""]
["7","040103001004","","回填砂","1.密实度要求 ：按设计及规范要求\r\n2.填方材料品种 ：按设计及规范要求\r\n3.填方来源、运距：投标人自行考虑\r\n4.其他：未尽事宜满足设计及现行技术、质量验收规范要求","m3","4000","","88.65",null,null,""]
["8","040503002006","","混凝土支墩","1.垫层材质、厚度 \r\n2.混凝土强度等级 C15\r\n3.预制混凝土构件运距：投标人自行考虑\r\n4.其他：未尽事宜满足设计及现行技术、质量验收规范要求","m3","16.8","","350.62",null,null,""]
["9","010103002007","","余方弃置","1.废弃料品种： 多余的管沟土石方\r\n2.运距：投标人自行考虑\r\n3.其他：未尽事宜满足设计及现行技术、质量验收规范要求","m3","7000","","13.45",null,null,""]
["10","040504001008","","砌筑水表井","1.垫层、基础材质及厚度： C15 厚0.1m\r\n2.砌筑材料品种、规格、强度等级 ：砖M7.5水泥砂浆砌筑\r\n3.勾缝、抹面要求： 内壁1:2水泥砂抹面\r\n4.砂浆强度等级、配合比： M7.5水泥砂浆砌筑\r\n5.混凝土强度等级 ：C15\r\n6.盖板材质、规格 ：按设计及规范要求\r\n7.井盖、井圈材质及规格 复合材质D700\r\n8.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","座","12","","2111.03",null,null,""]
["11","040504001009","","砌筑控制井","1.垫层、基础材质及厚度 C15 厚0.1m\r\n2.砌筑材料品种、规格、强度等级 砖M7.5水泥砂浆砌筑\r\n3.勾缝、抹面要求 内壁1:2水泥砂抹面\r\n4.砂浆强度等级、配合比 M7.5水泥砂浆砌筑\r\n5.混凝土强度等级 \r\n6.盖板材质、规格 \r\n7.井盖、井圈材质及规格 复合材质D700\r\n8.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","座","24","","1272.79",null,null,""]
["12","041001001010","","拆除砼路","1.名称：混凝土到路拆除\r\n2.混凝土路面厚度 ： 22mm\r\n3.含拆除垫层、基层及土石方开挖至设计深度\r\n4.其他：未尽事宜满足设计及现行技术、质量验收规范要求","m2","175","","88.57",null,null,""]
["13","040203007011","","水泥混凝土路面恢复","1.混凝土强度等级 ：C25\r\n2.混凝土路面厚度：0.22m\r\n3.含碎石垫层，基层等\r\n3.其他：未尽事宜满足设计及现行技术、质量验收规范要求","m2","175","","89.75",null,null,""]
["14","040501001028","","混凝土基础 C15","1.混凝土种类 ：商混\r\n2.混凝土强度等级：C15\r\n3.砼运输方式及场内、外运距:投标人自主确定\r\n4.砼现场泵送采用的机械种类及方式：投标人自主确定\r\n5.做法：满足设计及现行施工技术、质量验收规范要求","m3","162.75","","403.19",null,null,""]
["15","041102001001","","混凝土支墩模板","1.构件类型:混凝土支墩模板支拆\r\n2.支撑高度：按设计及规范要求\r\n3.模板材料：投标人自行考虑\r\n4.综合单价内应包含模板支架费及模板的安拆、维修、维护、运输等相关费用要求\r","m2","336","","27.89",null,null,""]
["16","041102002001","","井垫层模板","1.构件类型：井垫层模板支拆\r\n2.支撑高度：按设计及规范要求\r\n3.模板材料：投标人自行考虑\r\n4.综合单价内应包含模板支架费及模板的安拆、维修、维护、运输等相关费用要求\r\n","m2","213.3","","27.89",null,null,""]
["17","010401012037","","检查井升高","1.M5水泥砂浆砖砌体\r\n2.15厚1:3水泥砂浆内抹灰随抹\r\n3.井盖拆除安装\r\n4.运距由投标人自行考虑\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","m3","120","","487.28",null,null,""]
["18","011601001038","","砖砌体拆除","1.砖砌体或混凝土拆除\r\n2.井盖拆除安装\r\n3.建渣外运，运距由投标人自行考虑\r\n4.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","m3","60","","93.99",null,null,""]
[" "," ","","给水安装工程"," "," "," ",""," ",null,null,""]
["19","031001006012","","PE给水管 DE110","1.安装部位: 室外\r\n2.介质 :自来水\r\n3.材质、规格: PE管， De110\r\n4.连接形式: 热熔\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","m","12000","","92.05",null,null,""]
["20","031001006013","","PE给水管 DE63","1.安装部位 :室外\r\n2.介质 :自来水\r\n3.材质、规格: PE管， De63 1.6MPa\r\n4.连接形式: 热熔\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","m","24000","","44.69",null,null,""]
["21","031001006014","","PE给水管 DE32","1.安装部位 :室外\r\n2.介质: 自来水\r\n3.材质、规格: PE管， De32 1.6MPa\r\n4.连接形式: 热熔\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","m","24000","","20.93",null,null,""]
["22","031001006015","","PE给水管 DE20","1.安装部位: 室外\r\n2.介质 :自来水\r\n3.材质、规格 :PE管， De20 1.6MPa\r\n4.连接形式 :热熔\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r","m","20000","","21.54",null,null,""]
["23","031001006016","","低密度PE专用管 DE20","1.安装部位: 室外\r\n2.介质: 自来水\r\n3.材质、规格: 低密度PE专用管 DE20\r\n4.连接形式 :热熔\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","m","1000","","22.59",null,null,""]
["24","031003003017","","软密封闸阀 DN80","1.类型 :软密封闸阀\r\n2.材质 :铸铁\r\n3.规格、压力等级 :DN80 1.6MPa\r\n4.连接形式: 法兰\r\n5.焊接方法 :平焊\r\n6.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","个","12","","437.31",null,null,""]
["25","031003003018","","软密封闸阀 DN100\r\n0","1.类型 :软密封闸阀\r\n2.材质 :铸铁\r\n3.规格、压力等级 :DN100 1.6MPa\r\n4.连接形式 :法兰\r\n5.焊接方法: 平焊\r\n6.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","个","12","","549.30",null,null,""]
["26","031003001019","","软密封闸阀 DN50\r\n0","1.类型 :软密封闸阀\r\n2.材质 :铸铁\r\n3.规格、压力等级 :DN50 1.6MPa\r\n4.连接形式: 法兰\r\n5.焊接方法 :平焊\r\n6.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","个","12","","214.78",null,null,""]
["27","031003001020","","全铜闸阀 DN25","1.类型 :闸阀 DN25\r\n2.材质 :全铜\r\n3.规格、压力等级 1.6MPa\r\n4.连接形式 :螺纹\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r","个","240","","48.62",null,null,""]
["28","031003001021","","全铜闸阀 DN20","1.类型 :闸 阀 DN20\r\n2.材质:全铜\r\n3.规格、压力等级： 1.6MPa\r\n4.连接形式： 螺纹\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r","个","333","","36.42",null,null,""]
["29","031003001022","","止回阀DN80","1.类型 :止回阀\r\n2.规格、压力等级 ：DN80 1.6MPa\r\n3.连接形式 ：焊接\r\n4.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r","个","12","","775.90",null,null,""]
["30","031003001023","","电磁阀DN25","1.类型 ：电磁阀DN25\r\n2.规格、压力等级 1.6MPa\r\n3.连接形式： 螺纹\r\n4.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r","个","40","","733.84",null,null,""]
["31","031003001024","","电磁阀DN50","1.类型 ：电磁阀DN50\r\n2.规格、压力等级： DN50 1.6MPa\r\n3.连接形式 螺纹\r\n4.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","个","134","","911.81",null,null,""]
["32","031003001025","","电磁阀DN100","1.类型 ：电磁阀DN100\r\n2.规格、压力等级： DN100 1.6MPa\r\n3.连接形式 螺纹\r\n4.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","个","12","","1661.34",null,null,""]
["33","031003006026","","配套进口调压器 DN100","1.名称：配套进口调压器 \r\n2.规格、压力等级 ：DN100 1.6MPa\r\n3.连接形式 ：螺纹\r\n4.附件配置：按设计及规范要求\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","组","12","","6697.05",null,null,""]
["34","031003006027","","配套进口调压器 DN50","1.名称：配套进口调压器 \r\n2.规格、压力等级 ：DN50 1.6MPa\r\n3.连接形式 ：螺纹\r\n4.附件配置：按设计及规范要求\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","组","134","","3343.10",null,null,""]
["35","031003006027","","配套进口调压器 DN25 ","1.名称：配套进口调压器 \r\n2.规格、压力等级 ：DN50 1.6MPa\r\n3.连接形式 ：螺纹\r\n4.附件配置：按设计及规范要求\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","组","40","","1692.07",null,null,""]
["36","031003001028","","叠片式过滤器DN25","1.类型 :叠片式过滤器\r\n2.规格、压力等级 :DN25 1.6MPa \r\n3.连接形式 :螺纹\r\n4.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","个","40","","182.26",null,null,""]
["37","031003001029","","叠片式过滤器DN50","1.类型 :叠片式过滤器\r\n2.规格、压力等级 :DN50 1.6MPa\r\n3.连接形式 :螺纹\r\n4.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","个","134","","373.68",null,null,""]
["38","031003001030","","快速取水阀 DN25","1.类型 :快速取水阀 \r\n2.材质: 塑料\r\n3.规格、压力等级: DN251.6MPa\r\n4.连接形式 :螺纹\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","个","240","","101.54",null,null,""]
["39","031001001031","","镀锌钢管钢套管DN150","1.安装部位 ：室外\r\n2.介质 ：自来水\r\n3.规格、压力等级 ：DN150 1.6MPa\r\n4.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r","m","350","","99.00",null,null,""]
["40","031003001032","","十字雾化喷头","1.类型 ：十字雾化喷头\r\n2.材质： 塑料\r\n3.规格、压力等级： WP13101 Q=31-40L/H 射程1.0-1.1m\r\n4.连接形式 ：插接 （D4mm毛管连接、配套支架等配件）\r\n5.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r","套","2500","","41.68",null,null,""]
["41","050103002033","","进口T5喷头","1.管道附件、阀门、喷头品种、规格： 地埋式喷头T5（进口） 射程9-14.2m，Q=1-1.45m3/h\r\n2.管道附件、阀门、喷头固定方式 ：配套千秋架安装\r\n3.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n","个","2100","","149.16",null,null,""]
["42","030503006034","","雨量传感器","1.名称 ：雨量传感器\r\n2.规格：按设计要求\r\n3.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r","套","12","","373.88",null,null,""]
["43","030404019035","","控制器安装","1.名称 ：控制器安装\r\n2.型号 ：按设计要求\r\n3.其他：未尽事宜满足设计及现行技术、质量验收规范要求\r\n\r\n","套","186","","930.32",null,null,""]
["合　　计（大写：                                                  ）","","","","","","","","",""]